# Air Knife Bottle Dryer

### Description

In modern times, with an ever increasing demand for all goods, high speed production lines are becoming norms of the day. Some of other concerns of modern day production lines are cost effectiveness, better quality, better hygiene, better self-life, better packaging, better appearance, faster production, lesser handling, lesser pollution, interfacing with other production inputs etc. To address these demands there are variety of innovative tools available. Among them AIR KNIFE is one such tool which has made difference in many fields and constantly finding new applications. AIR KNIFE SYSTEM is a non-contact method of removing unwanted surface liquid, moisture, dirt, coatings, contamination, debris, heat, static charge etc. During manufacturing process of predominantly conveyed (moving) articles or parts. In certain applications where longer / deeper reach of high velocity air is required nozzles could also be used. Drying with low pressure Air Knife System has been known to cut cost by 80% compared with Thermal Drying and Compressed air system. An effective working Air Knife System can be assembled using standard single or multiple Air Knife’s, located strategically. For certain applications combination of Air Knife’s with Air Nozzle’s will bring desired results. Air Knife’s and Nozzles are available in different sizes, lengths and shapes. Special Filters are available to meet most stringent standard for Food, Pharmaceuticals, Electronic or similar applications. Various types of manifolds like Nozzle Manifold, Cap Dryer, Spider Manifold.

### Applications

1. Bottles/Cans Drying. 2. Bottle Label Drying. 3. Food packets/Pouch. 4. Beverage/Jam/Pickle. 5. Vegetable Drying. 6. Bakery/Confectionary Products. 7. PCB Drying. 8. Food Handling Tray. 9. Adhesive Drying. 10. Glass/ Plastic Sheet. 11. Paper Drying.

### Features

1. Stainless Steel Enclosure For Blower. 2. Aluminium casted Blower. 3. Aluminium Casted Air Knife. 4. Machine is easy to install. 5. Easy to adjust Air Knife height as per required.

Air Knife Size | W= 80MM, L= 400 or as required)
Machine Size | 0.75 or 1H.P. / 440V / 3PH
Electricals | 3 PHASE, 220V
Air Flow Pressure (Kpa) | 5.15 – 25.5
Air Flow Rate (M3min) | 0.58 – 7.5

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry