# Piston Filling Machine

### Description

1. Accuracy ± 1 % in single doze. 2. Rigid vibration free construction for trouble free performance. 3. Stainless Steel elegantly matt finished body. 4. Elegant and easy control panel for total control on operation. 5. Minimum change over time , from one size to another container or fill size. 6. Reciprocating Filling nozzle with self centering device to avoid foaming. 7. No container No Filling system-to avoid Spillage. 8. Synchronized A.C. drives for conveyor & main drive

### Applications

1. Semi-Viscous & Viscous Liquid. 2. Lube Oil. 3. Edible Oil. 4. Syrup. 5. Pharmaceuticals. 6. Juice.

1) | Modal no. | RALF-100(4 HEAD) RALF-150(6 HEAD)
2) | Output/Hour | 2500 To 6000 3500 To 9000
3) | Electric motor | Main machine 1 HP / 440 Volts / 3 Ph / 50 Hz
|  | Conveyor 0.5 HP / 440 Volts / 3 Ph / 50 Hz
4) | Container size | Ø 30 mm To Ø 100 mm, Maximum Height 210 mm
5) | Fill size | 10 ml. To 500 ml. (With the help of required change part))
| 6) | Dimension | 2035mm (L) X 1050mm (W) X 1400mm (H)

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry