# Batch Coding Machine

### Description

These coders are ideal for Automatic High Speed Coding on large quantities of labels. It delivers high quality multi-line printing at production speeds of 250 impressions / minute. The labels or pouches are stacked on the slanting tray (Dispenser) for feeding, automatically picked up by the pick-up rubber friction insert, fed to the printing roller one by one via guide track and timing chain & stacked back in the collection tray automatically at very high speeds. This system is similar to rotary letterpress. The oscillating roller disperses an even thickness of ink film on the inking roller and the inking roller transfers the ink to the stereos & finally the image is transferred to the substrate. This cycle is continuously running at high speed with clear & sharp impressions. The system is totally mechanically synchronized so that the printing is done exactly at the same location automatically.

Subtrate | Labels Or Pouches
Subtrate Size | 40X20MM TO 200X150MM
Printing Area | 6 TO 8 LINES
Printing Speed | 250 Imprints Per Minute
Use Of Letter | Rubber Stereo
Impressions | 15000 PER 20ML
Dimensions | 800X425X490MM (LXWXH)

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry