# Steam Shrink Wrapping Machine

### Description

Heat shrink tunnels are designed to work with both tamper evident bands and sleeve labels. We produces convective, radiant, and steam heat shrink tunnels that offer optimum shrink performance for a wide range of standard product sizes while using minimum space. Special exhauster fan for no steam loss. It is widely used in Bottling Industries, Food, Beverage, Pharmaceuticals, Cosmetics, ETC.

### Features

1. MOC - Stainless Steel 304. 2. Smooth Operation & Easy Maintenance. 3. High Speed Special Impellor. 4. Pressure Reducing Valves. 5. Pressure and Temperature Gauges. 6. Height Adjustable Leveling Legs. 7. Special Exhaust Fan For No Steam Loss. 8. Moisture Collection: Integrated Drip Tray. 9. Double Shell Design Keeps Outer Temperature Of Machine Cooler. 10. Tunnels Are Available In Different Sizes. 11. Full Shrinking is Quickly Accomplished In Only Three Seconds. 12. MS Construction also available.

Tunnel Area | L= Unlimited X 125 X 300mm (Lxwxh)
Machine Size | 1260 X 445 X 450mm (Lxwxh)
Conveyor Length | 10 Ft
Conveyor Motor | 1 H.P, 3ph
Exhaust Fan | 220V
Packing Material | Pvc, Ld, Poly-Olyfin Or Any Other Shrinkable Film
Output | 500 Bpm (Upto)

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry