# Electric Shrink Wrapping Machine

### Description

Very efficient machine, all around close design ensures less heat loss thus less electricity consumption. Heavy-duty conveyor system, which is having insulated surface to avoid any damage to product or shrink sleeve. High speed blower system with continuous rating. High quality heating element. Machine can be attached with any other packing machine or operation to give online application. It is widely use in Packaging Industries, Bottling Industries, Food, Pharmaceuticals, Cosmetics, ETC.

### Features

1. Moc - Stainless Steel 304> 2. Smooth Operation & Easy Maintenance. 3. High Speed Special Impellor. 4. Separate Control Panel Box For Protection. 5. Digital Temperature Controller. 6. Height Adjustable Leveling Legs. 7. Energy Efficient Design. 8. Tunnels Are Available In Different Sizes. 9. Full Shrinking is Quickly Accomplished In Only Three Seconds.

Tunnel Area | L= Unlimited,W=125mm, H=330mm
Machine Size | 775 X 420 X 720mm (Lxwxh)
Heater | 6 Kw, 220v
Impellor Motar | 0.5 Hp
Packing Material | Pvc, Ld, Poly-Olyfin Or Any Other Shrinkable Film

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry