# P.P. Cap Sealing Machine

### Description

It is a Semi-Automatic Capping Machine is known for its high performance and efficiency. Our Semi-Automatic Capping Machine remains in use for a long time without any chance of corrosion. Head comes down automatically seal and go up and it can be operated by foot switch also. It has two threading and two sealing rollers can seal different diameters and heights of ROPP Caps (Standard Deep Drawn, Semi Deep Drawn, extra Deep Drawn caps etc.)

### Product Detail

1) | Application. | Sealing Of Ropp, Guala, Screw Caps, Etc
2) | Type of bottle | GLASS/PET
3) | Working height | Adjustable for different shape & size of bottle
| 4) | Power | 1HP 3 PH
5) | Moc-Base | Ms powder coated
| 6) | Moc-Head | High grade casting powder coated | 7) | Output | 70-80 BPM) | 8) | Dimensions | (L X W X H)

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurdeep Singh Anand +91-98-10-179425
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry