# Semi Automatic Filling Machine

### Description

Rattan Semi-Automatic Liquid Filling Machine is very simple, Piston base volumetric filler. It gives very accurate volumes with remarkable speed. It is widely use in Pharmaceutical, Chemical, Paint, Cosmetic, Oil, Liquor Industries.

### Features

1. Accuracy ± 1 % in single doze. 2. Rigid vibration free construction for trouble free performance. 3. Stainless Steel elegantly matt finished body. 4. Elegant and easy control panel for total control on operation. 5. Portable And Compact Design. 6. All Contact Parts Are Of SS 304/316 Grade. 7. Very Easy To Change Over. 8. Maintenance Free Modal

### Applications

1. Semi-Viscous & Viscous Liquid 2. Lube Oil. 3. Edible Oil. 4. Vegetable Oil. 5. Mustard Oil. 6. Syrup. 7. Pharmaceuticals. 8. Juice, etc.

### Syringe Range

1. 2ML to 10ML. 2. 10ML to 30ML. 3. 30ML TO 100ML. 4. 50ML TO 250ML. 5. 100ML TO 500ML. 6. 500ML TO 1000ML

1) | Filling range | 2ML to 1Lt. (with some suitable change over)
2) | Motor | 0.75 or 1H.P. / 440V / 3PH
3) | Output | 700 to 2000 BPH (depend on volume & viscosity of the product)
4) | Fill accuracy | +- 1%
5) | Dimension | 360 X 460 X 650MM
6) | Net weight | 110 kg. (approx.)

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry