# Turn Table

### Description

Stainless steel scrambler & un-scrambler, which is familiar as turn table. This is built on SS square frame, solid guide rail & reduction gear box for jerk less & noiseless performance. Turntable is useful to ensure total synchronization, uniform flow of container and to take a turn at 90 degree to suit different machine and purpose in automatic liquid line.

### Options

Container inputs in turn table by manually or automatic will rotate on disk of turn table and exit through outlet, during rotation of container will guided by a SS strip, which will guide the container towards outlet path.

### Features

1. Accuracy ± 1 % in single doze. 2. Construction Stainless Steel 304 quality. 3. AC Frequency Drive. 4. Special self-aligning bearings ensure smooth and trouble free operation. 5. Heavy-duty conveyor system. 6. Suitable for different type of container. 7. S.S. elegantly matt finished body. 8. Reduction gears ensure jerk free and noiseless operation. 8. Matt Finished body.

Modal No. | RTT-30 | RTT-36 | RTT-42
Direction | Clockwise / Anti clock wise as per requirement | - | -
Electric Motor | 0.5 HP/415 V/50 Hz | - | -
Height Of Disk | 860MM to 910MM | - | -
Machine Dimension | 780x780x1160 | 925x925x1160 | 1076x1076x1160
Weight | 80 | 100 | 130
Electric Load | 1KW | - | -

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry