# Sticker Labeling Machine

### Description

Output 80 to 100 Vials/Min. Depending upon label size and Vial dia(LSL 100-Stepper Motor , PLC , HMI). Suitable for all online inject and contact coding system. No oil / No Greece required for maintainance Purpose. Power Characteristics : 230 V, 1 Phase, 50 Hz. Overall Dimension : L - 1600mm, W- 600mm, H: 1200mm. Label role Core diameter 75/ 76mm.

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry