# Tunnel Washing

### Description

The Tunnel Washer Machine is most ideal for Round Bottles and finds wide application in Liquor, Mineral Water, Pharmaceuticals, Juice, Food Industries. The automatic loading arrangement facilities loading of bottles on to SS wire mesh conveyor or bottles are pushed manually From feed table. This saves manpower as bottles are fed up into pockets automatically. The automatic unloading mechanism consists of unloading bottle on to a wire mesh conveyor which continues on to turn table. Three cycle rinsing allows flexibilities of various rinse cycles such as fresh water, DM water etc. As per the rinsing requirement of bottles. All the pumps are made of SS and all the water contact parts are made of SS 304 on a heavy base of MS painted structure. The total rinsing cycle is smooth and limit switches/sensors are inbuilt at every stage to sense bottle, reversal or bottle obstruction and stop the machine. The quality of rinsing is ensured through 3 sets of inner and 3 sets of outer nozzles accurately placed to direct the jet at center of the bottle and the bottle comes out with water totally drained with minimum droplets of water which can also be removed by providing final rinse by compressed air or hot air blowing (optional).

### Features

1. Save Manpower. 2. Automatic Unloading Mechanism. 3. Made up of SS and other fitting parts are of SS 304. 4. Nozzle set’s - 3 sets of Inner & 3 sets of Outer.

MODELS(NO.OF POCKETS) | LENGTH (MM) | WIDTH (MM) | HEIGHT (MM) | OUTPUT (BPM) | RINSING CYCLE
--- | --- | --- | --- | --- | ---
5 | 3660 | 1525 | 1525 | 40-60 | 2 STAGE
10 | 4270 | 1830 | 1525 | 100-120 | 3 STAGE
14 | 4270 | 2585 | 1525 | 120-150 | 3 STAGE
20 | 4270 | 2745 | 1525 | 200-240 | 3 STAGE

### Our Location

### Navigation

- Bottling Line
- Liquor Filling Machine
- Wine Plant
- Distillery Plant
- Wine Tank

### Address

- info@rsanand.com | ksanand@rsanand.com
- Mr.Gurmeet Singh Anand +91 9810636797
- Mr.Karan Singh Anand +91-8800620033

Send Inquiry